**Record Description**

**Subject:**

2015 BPVC, Section III, Division 2, CC-3532.1.5; A typo

**Proposal:**

Correct a typo in CC-3532.1.5.

**Explanation**

There appears to be a typo in CC-3532.1.5. The second “CC-4334” should be “CC-4333.”

|  |  |
| --- | --- |
| ASME BPVC, Sec. III, Div. 2, CC-3532.1.5 (Current) | ASME BPVC, Sec. III, Div. 2, CC-3532.1.5 (Proposed) |
| **CC-3532.1.5 Splices in Tension Tie Members.**  Splices shall be made with a welded butt splice in accordance with CC-4334 or a positive mechanical connection in accordance with CC-4334 and be staggered at least 1.3**ld.** | **CC-3532.1.5 Splices in Tension Tie Members.**  Splices shall be made with a welded butt splice in accordance with CC-4334 or a positive mechanical connection in accordance with CC-4333 and be staggered at least 1.3**ld.** |