
Subject: Mandatory Appendix II Amplitude Control Linearity

Edition/ Addenda: ASME BPV V 2015 and Later

Paragraph/ Fig. / Table No.: Article 4 Mandatory Appendix II (II-440)

Action: To fix Table II-440 (2015 and later editions of the Code) the RED column in the upper table needs to be replaced with the BLUE column of the lower table.

**2015 and later table (incorrect)**



**Prior to 2015 table (corrected)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Indication Set at %  Of Full Screen | dB Control  Change | Indication Limits  % Of Full Screen |  |
|  | **80%** | -6 dB | 32% to 48% |  |
|  | **80%** | -12 dB | 16% to 24% |  |
|  | **40%** | +6 dB | 64% to 96% |  |
|  | **20%** | +12 dB | 64% to 96% |  |