***Record 14-1556 Errata***

***NCA-5300  Responsibilities of the Authorized Inspection Agency***

The responsibilities of the Authorized Inspection Agency shall include but not necessarily be limited to those given in (a) through (k) below.

*(a)* Maintain a staff of Authorized Nuclear Inspectors and Authorized Nuclear Inspector Supervisors ([NCA-5123](%5Cl%22asme_5F_30_2D7918_2D_3988)).

*(b)* Make agreements with Certificate Holders and Owners for inspection service ([NCA-5121 and NCA-8130](%5Cl%22asme_5F_30_2D7918_2D_999892041%22)). Notify the Society whenever such agreements are terminated ([NCA-5121](%5Cl%22asme_5F_30_2D7918_2D_999892041%22)).

*(c)* Provide for participation in the Society’s review of the applicant’s Quality Assurance Program ([NCA-5125](%5Cl%22asme_5F_30_2D7918_2D_1800713722%22)).

*(d)* Provide for the review and acceptance of any proposed modifications to Quality Assurance Manuals before they are put into effect ([NCA-5125](%5Cl%22asme_5F_30_2D7918_2D_1800713722%22)).

*(e)* Review and accept the Certificate Holder’s method of securing the nameplate to components to which, because of size or other considerations, the nameplate cannot be directly attached [[NCA-8220(b)](%5Cl%22asme_5F_30_2D7918_2D_2786621660%22)].

*(f)* Review and accept the Certificate Holder’s alternative method of identification, including the unique method of marking of components to which, because of size or other considerations, nameplates cannot be directly attached [[NCA-8220(b)](%5Cl%22asme_5F_30_2D7918_2D_2786621660%22)].

*(g)* Review and accept the Certificate Holder’s alternative method of marking of parts, appurtenances, supports, and piping subassemblies ([NCA-8230](%5Cl%22asme_5F_30_2D7918_2D_2534745041%22)).

*(h)* Review and accept the Certificate Holder’s provisions of positive identification and traceability of items from which nameplates are removed [ NCA-8240

*(i)* Determine by agreement with the Certificate Holder the sequence for stamping and the completion of the Code Data Report [[NCA-8310(c)](%5Cl%22asme_5F_30_2D7918_2D_4180400040%22)].

*(j)* Review and accept the Certificate Holder’s procedure for providing traceability of parts for piping subassemblies which are furnished without stamping ( NCA-8330).

*(k)* And all other duties specifically required in ASME QAI‐1, Qualification for Authorized Inspection, as applicable.